(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A5")
	(title_block
		(title "Basic ATTiny on a Breadboard")
		(date "2024-04-02")
		(rev "0.0.1")
		(company "carlynorama")
		(comment 1 "Inputs: software determined SPST M, reset SPST M")
		(comment 2 "Outputs: power supply on LED, software determined LED")
		(comment 4 "Circuit for an ATTiny on a breadboard with a \"header\"  for the programmer.")
	)
	(lib_symbols
		(symbol "Connector:AVR-ISP-6"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J1"
				(at -8.89 2.5401 0)
			)
			(property "Value" "AVR-ISP-6"
				(at -8.89 0.0001 0)
			)
			(property "Footprint" ""
				(at -6.35 1.27 90)
			)
			(property "Datasheet" " ~"
				(at -32.385 -13.97 0)
			)
			(property "Description" "Atmel 6-pin ISP connector"
				(at 0 0 0)
			)
			(property "ki_keywords" "AVR ISP Connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*"
				(at 0 0 0)
			)
			(symbol "AVR-ISP-6_0_1"
				(rectangle
					(start -7.62 10.16)
					(end 7.62 -7.62)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -2.667 -6.858)
					(end -2.413 -7.62)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -2.667 10.16)
					(end -2.413 9.398)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.62 -2.413)
					(end 6.858 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.62 0.127)
					(end 6.858 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.62 2.667)
					(end 6.858 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.62 5.207)
					(end 6.858 4.953)
					(fill
						(type none)
					)
				)
			)
			(symbol "AVR-ISP-6_1_1"
				(pin passive line
					(at 10.16 2.54 180)
					(length 2.54)
					(name "MISO")
					(number "1")
				)
				(pin passive line
					(at -2.54 -10.16 90)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "SCK")
					(number "3")
				)
				(pin passive line
					(at 10.16 5.08 180)
					(length 2.54)
					(name "MOSI")
					(number "4")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "~{RST}")
					(number "5")
				)
				(pin passive line
					(at -2.54 12.7 270)
					(length 2.54)
					(name "GND")
					(number "6")
				)
			)
		)
		(symbol "Connector:Conn_01x02_Socket"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Socket"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Socket_1_1"
				(arc
					(start 0 -2.032)
					(mid -0.5058 -2.54)
					(end 0 -3.048)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -2.54) (xy -0.508 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy -0.508 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0.508)
					(mid -0.5058 0)
					(end 0 -0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "Device:C_Polarized"
			(pin_numbers hide)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_Polarized"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Polarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "CP_*"
				(at 0 0 0)
			)
			(symbol "C_Polarized_0_1"
				(rectangle
					(start -2.286 0.508)
					(end 2.286 1.016)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 2.286) (xy -0.762 2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.794) (xy -1.27 1.778)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.508)
					(end -2.286 -1.016)
					(fill
						(type outline)
					)
				)
			)
			(symbol "C_Polarized_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:D"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "D"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Diode"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
				(at 0 0 0)
			)
			(symbol "D_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "D_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "MCU_Microchip_ATtiny:ATtiny85-20P"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U2"
				(at -14.224 -3.048 0)
			)
			(property "Value" "ATtiny85-20P"
				(at -14.478 -5.334 0)
			)
			(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
				(at 0 0 0)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
				(at 0 0 0)
			)
			(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm*"
				(at 0 0 0)
			)
			(symbol "ATtiny85-20P_0_1"
				(rectangle
					(start -12.7 12.7)
					(end 12.7 -12.7)
					(fill
						(type background)
					)
				)
			)
			(symbol "ATtiny85-20P_1_1"
				(pin bidirectional line
					(at 15.24 8.89 180)
					(length 2.54)
					(name "~{RESET}/PB5")
					(number "1")
				)
				(pin bidirectional line
					(at -15.24 3.81 0)
					(length 2.54)
					(name "XTAL1/PB3")
					(number "2")
				)
				(pin bidirectional line
					(at -15.24 1.27 0)
					(length 2.54)
					(name "XTAL2/PB4")
					(number "3")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "AREF/PB0")
					(number "5")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "PB1")
					(number "6")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "PB2")
					(number "7")
				)
				(pin power_in line
					(at -7.62 15.24 270)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
		)
		(symbol "Regulator_Linear:LM7805_TO220"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -3.81 3.175 0)
			)
			(property "Value" "LM7805_TO220"
				(at 0 3.175 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
				(at 0 5.715 0)
			)
			(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
				(at 0 -1.27 0)
			)
			(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"
				(at 0 0 0)
			)
			(property "ki_keywords" "Voltage Regulator 1A Positive"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?220*"
				(at 0 0 0)
			)
			(symbol "LM7805_TO220_0_1"
				(rectangle
					(start -5.08 1.905)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "LM7805_TO220_1_1"
				(pin power_in line
					(at -7.62 0 0)
					(length 2.54)
					(name "VI")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_out line
					(at 7.62 0 180)
					(length 2.54)
					(name "VO")
					(number "3")
				)
			)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 63.5 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 68.58 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 119.38 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 40.64 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 63.5 62.23) (xy 64.77 62.23)
		)
	)
	(wire
		(pts
			(xy 76.2 118.11) (xy 76.2 120.65)
		)
	)
	(wire
		(pts
			(xy 54.61 109.22) (xy 54.61 114.3)
		)
	)
	(wire
		(pts
			(xy 25.4 100.33) (xy 30.48 100.33)
		)
	)
	(wire
		(pts
			(xy 119.38 45.72) (xy 119.38 48.26)
		)
	)
	(wire
		(pts
			(xy 119.38 35.56) (xy 119.38 38.1)
		)
	)
	(wire
		(pts
			(xy 104.14 72.39) (xy 104.14 74.93)
		)
	)
	(wire
		(pts
			(xy 119.38 48.26) (xy 119.38 53.34)
		)
	)
	(wire
		(pts
			(xy 74.93 55.88) (xy 74.93 62.23)
		)
	)
	(wire
		(pts
			(xy 68.58 100.33) (xy 62.23 100.33)
		)
	)
	(wire
		(pts
			(xy 119.38 64.77) (xy 143.51 64.77)
		)
	)
	(wire
		(pts
			(xy 54.61 107.95) (xy 54.61 109.22)
		)
	)
	(wire
		(pts
			(xy 68.58 97.79) (xy 68.58 100.33)
		)
	)
	(wire
		(pts
			(xy 25.4 102.87) (xy 25.4 114.3)
		)
	)
	(wire
		(pts
			(xy 68.58 109.22) (xy 54.61 109.22)
		)
	)
	(wire
		(pts
			(xy 76.2 97.79) (xy 76.2 100.33)
		)
	)
	(wire
		(pts
			(xy 62.23 53.34) (xy 64.77 53.34)
		)
	)
	(wire
		(pts
			(xy 62.23 62.23) (xy 63.5 62.23)
		)
	)
	(wire
		(pts
			(xy 156.21 72.39) (xy 156.21 74.93)
		)
	)
	(wire
		(pts
			(xy 156.21 35.56) (xy 156.21 49.53)
		)
	)
	(wire
		(pts
			(xy 40.64 100.33) (xy 46.99 100.33)
		)
	)
	(wire
		(pts
			(xy 68.58 100.33) (xy 68.58 101.6)
		)
	)
	(wire
		(pts
			(xy 76.2 107.95) (xy 76.2 110.49)
		)
	)
	(wire
		(pts
			(xy 40.64 109.22) (xy 54.61 109.22)
		)
	)
	(wire
		(pts
			(xy 119.38 62.23) (xy 143.51 62.23)
		)
	)
	(wire
		(pts
			(xy 88.9 55.88) (xy 74.93 55.88)
		)
	)
	(wire
		(pts
			(xy 96.52 35.56) (xy 96.52 41.91)
		)
	)
	(wire
		(pts
			(xy 50.8 62.23) (xy 50.8 53.34)
		)
	)
	(wire
		(pts
			(xy 72.39 53.34) (xy 88.9 53.34)
		)
	)
	(wire
		(pts
			(xy 40.64 100.33) (xy 40.64 101.6)
		)
	)
	(wire
		(pts
			(xy 50.8 53.34) (xy 54.61 53.34)
		)
	)
	(wire
		(pts
			(xy 38.1 100.33) (xy 40.64 100.33)
		)
	)
	(wire
		(pts
			(xy 134.62 53.34) (xy 135.89 53.34)
		)
	)
	(wire
		(pts
			(xy 50.8 35.56) (xy 50.8 53.34)
		)
	)
	(wire
		(pts
			(xy 63.5 62.23) (xy 63.5 68.58)
		)
	)
	(wire
		(pts
			(xy 119.38 59.69) (xy 143.51 59.69)
		)
	)
	(wire
		(pts
			(xy 143.51 48.26) (xy 143.51 57.15)
		)
	)
	(wire
		(pts
			(xy 119.38 48.26) (xy 143.51 48.26)
		)
	)
	(wire
		(pts
			(xy 54.61 62.23) (xy 50.8 62.23)
		)
	)
	(wire
		(pts
			(xy 119.38 53.34) (xy 124.46 53.34)
		)
	)
	(text "Board Power Supply Circuit"
		(exclude_from_sim no)
		(at 53.086 127 0)
	)
	(text "Human Interface"
		(exclude_from_sim no)
		(at 70.612 38.862 0)
	)
	(text "Programming"
		(exclude_from_sim no)
		(at 138.176 38.608 0)
	)
	(symbol
		(lib_id "Device:D")
		(at 34.29 100.33 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 34.036 94.234 0)
		)
		(property "Value" "1N4004"
			(at 34.036 97.028 0)
		)
		(property "Footprint" "Diode_THT:D_DO-15_P15.24mm_Horizontal"
			(at 34.29 100.33 0)
		)
		(property "Datasheet" "~"
			(at 34.29 100.33 0)
		)
		(property "Description" "Diode"
			(at 34.29 100.33 0)
		)
		(property "Sim.Device" "D"
			(at 34.29 100.33 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 34.29 100.33 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 120.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 76.2 127 0)
		)
		(property "Value" "GND"
			(at 76.2 125.73 0)
		)
		(property "Footprint" ""
			(at 76.2 120.65 0)
		)
		(property "Datasheet" ""
			(at 76.2 120.65 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 76.2 120.65 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 68.58 53.34 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D3"
			(at 68.326 49.022 0)
		)
		(property "Value" "Digital Output (5.0mm LED)"
			(at 70.1675 49.53 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 68.58 53.34 0)
		)
		(property "Datasheet" "~"
			(at 68.58 53.34 0)
		)
		(property "Description" "Light emitting diode"
			(at 68.58 53.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulator_Linear:LM7805_TO220")
		(at 54.61 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 54.61 93.98 0)
		)
		(property "Value" "LM7805"
			(at 54.61 96.52 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 54.61 94.615 0)
		)
		(property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF"
			(at 54.61 101.6 0)
		)
		(property "Description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"
			(at 54.61 100.33 0)
		)
		(pin "3")
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 25.4 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 25.4 120.65 0)
		)
		(property "Value" "GND"
			(at 25.4 119.38 0)
		)
		(property "Footprint" ""
			(at 25.4 114.3 0)
		)
		(property "Datasheet" ""
			(at 25.4 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 25.4 114.3 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 76.2 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 76.2 101.6 0)
		)
		(property "Value" "+5V"
			(at 76.2 92.71 0)
		)
		(property "Footprint" ""
			(at 76.2 97.79 0)
		)
		(property "Datasheet" ""
			(at 76.2 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 76.2 97.79 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 63.5 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 63.5 74.93 0)
		)
		(property "Value" "GND"
			(at 63.5 73.66 0)
		)
		(property "Footprint" ""
			(at 63.5 68.58 0)
		)
		(property "Datasheet" ""
			(at 63.5 68.58 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 63.5 68.58 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:AVR-ISP-6")
		(at 153.67 59.69 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 162.56 62.2301 0)
		)
		(property "Value" "AVR-ISP-6"
			(at 162.56 59.6901 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 160.02 60.96 90)
		)
		(property "Datasheet" " ~"
			(at 186.055 45.72 0)
		)
		(property "Description" "Atmel 6-pin ISP connector"
			(at 153.67 59.69 0)
		)
		(pin "3")
		(pin "1")
		(pin "5")
		(pin "6")
		(pin "4")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 96.52 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 96.52 39.37 0)
		)
		(property "Value" "+5V"
			(at 96.52 30.48 0)
		)
		(property "Footprint" ""
			(at 96.52 35.56 0)
		)
		(property "Datasheet" ""
			(at 96.52 35.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 96.52 35.56 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 129.54 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW1"
			(at 129.54 55.88 0)
		)
		(property "Value" "Reset Switch (SPST Push)"
			(at 129.54 48.26 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm"
			(at 129.54 48.26 0)
		)
		(property "Datasheet" "~"
			(at 129.54 48.26 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 129.54 53.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 54.61 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 54.61 120.65 0)
		)
		(property "Value" "GND"
			(at 54.61 119.38 0)
		)
		(property "Footprint" ""
			(at 54.61 114.3 0)
		)
		(property "Datasheet" ""
			(at 54.61 114.3 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 54.61 114.3 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 58.42 62.23 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R4"
			(at 58.42 65.278 90)
		)
		(property "Value" "10kΩ"
			(at 58.42 67.31 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal"
			(at 58.42 64.008 90)
		)
		(property "Datasheet" "~"
			(at 58.42 62.23 0)
		)
		(property "Description" "Resistor"
			(at 58.42 62.23 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 50.8 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 50.8 39.37 0)
		)
		(property "Value" "+5V"
			(at 50.8 30.48 0)
		)
		(property "Footprint" ""
			(at 50.8 35.56 0)
		)
		(property "Datasheet" ""
			(at 50.8 35.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 50.8 35.56 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 53.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 142.24 53.34 0)
		)
		(property "Value" "GND"
			(at 133.858 55.88 90)
		)
		(property "Footprint" ""
			(at 135.89 53.34 0)
		)
		(property "Datasheet" ""
			(at 135.89 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 135.89 53.34 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 76.2 104.14 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 80.01 105.7274 90)
		)
		(property "Value" "5.0mm Power Indicator LED"
			(at 80.01 106.9974 90)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 76.2 104.14 0)
		)
		(property "Datasheet" "~"
			(at 76.2 104.14 0)
		)
		(property "Description" "Light emitting diode"
			(at 76.2 104.14 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 76.2 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 78.74 113.0299 0)
		)
		(property "Value" "330Ω"
			(at 78.74 115.5699 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal"
			(at 74.422 114.3 90)
		)
		(property "Datasheet" "~"
			(at 76.2 114.3 0)
		)
		(property "Description" "Resistor"
			(at 76.2 114.3 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 69.85 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW2"
			(at 69.85 65.024 0)
		)
		(property "Value" "Digital Input (SPST Push)"
			(at 69.85 57.15 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm_H5mm"
			(at 69.85 57.15 0)
		)
		(property "Datasheet" "~"
			(at 69.85 57.15 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 69.85 62.23 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Polarized")
		(at 68.58 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 69.596 108.458 0)
		)
		(property "Value" "1uF"
			(at 69.596 110.744 0)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 69.5452 109.22 0)
		)
		(property "Datasheet" "~"
			(at 68.58 105.41 0)
		)
		(property "Description" "Polarized capacitor"
			(at 68.58 105.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Socket")
		(at 20.32 102.87 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J2"
			(at 22.098 105.41 0)
		)
		(property "Value" "External Power Connection"
			(at 27.686 96.774 0)
		)
		(property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
			(at 20.32 102.87 0)
		)
		(property "Datasheet" "~"
			(at 20.32 102.87 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 20.32 102.87 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 156.21 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 156.21 39.37 0)
		)
		(property "Value" "+5V"
			(at 156.21 30.48 0)
		)
		(property "Footprint" ""
			(at 156.21 35.56 0)
		)
		(property "Datasheet" ""
			(at 156.21 35.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 156.21 35.56 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Microchip_ATtiny:ATtiny85-20P")
		(at 104.14 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 111.76 71.882 0)
		)
		(property "Value" "ATtiny85-20P"
			(at 111.506 74.168 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 104.14 57.15 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 104.14 57.15 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
			(at 104.14 57.15 0)
		)
		(pin "2")
		(pin "8")
		(pin "7")
		(pin "3")
		(pin "6")
		(pin "1")
		(pin "4")
		(pin "5")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 104.14 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 104.14 81.28 0)
		)
		(property "Value" "GND"
			(at 104.14 80.01 0)
		)
		(property "Footprint" ""
			(at 104.14 74.93 0)
		)
		(property "Datasheet" ""
			(at 104.14 74.93 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 104.14 74.93 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 58.42 53.34 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 58.42 48.006 90)
		)
		(property "Value" "330Ω"
			(at 58.42 50.546 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal"
			(at 58.42 51.562 90)
		)
		(property "Datasheet" "~"
			(at 58.42 53.34 0)
		)
		(property "Description" "Resistor"
			(at 58.42 53.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 119.38 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 119.38 39.37 0)
		)
		(property "Value" "+5V"
			(at 119.38 30.48 0)
		)
		(property "Footprint" ""
			(at 119.38 35.56 0)
		)
		(property "Datasheet" ""
			(at 119.38 35.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 119.38 35.56 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Polarized")
		(at 40.64 105.41 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 39.624 108.458 0)
		)
		(property "Value" "10uF"
			(at 39.878 110.998 0)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 39.6748 109.22 0)
		)
		(property "Datasheet" "~"
			(at 40.64 105.41 0)
		)
		(property "Description" "Polarized capacitor"
			(at 40.64 105.41 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 68.58 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 68.58 101.6 0)
		)
		(property "Value" "+5V"
			(at 68.58 92.71 0)
		)
		(property "Footprint" ""
			(at 68.58 97.79 0)
		)
		(property "Datasheet" ""
			(at 68.58 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 68.58 97.79 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 119.38 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 121.92 40.6399 0)
		)
		(property "Value" "10kΩ"
			(at 121.92 43.1799 0)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal"
			(at 117.602 41.91 90)
		)
		(property "Datasheet" "~"
			(at 119.38 41.91 0)
		)
		(property "Description" "Resistor"
			(at 119.38 41.91 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 156.21 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 156.21 81.28 0)
		)
		(property "Value" "GND"
			(at 156.21 80.01 0)
		)
		(property "Footprint" ""
			(at 156.21 74.93 0)
		)
		(property "Datasheet" ""
			(at 156.21 74.93 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 156.21 74.93 0)
		)
		(pin "1")
		(instances
			(project "AttinyBasicBoard"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)