(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "ItsyBitsyM0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U1"
			(at -0.635 1.27 0)
		)
		(property "Value" "ItsyBitsy M0 Express"
			(at -0.635 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://learn.adafruit.com/introducing-itsy-bitsy-m0"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ItsyBitsyM0_0_1")
		(symbol "ItsyBitsyM0_1_1"
			(text "DotStar\nCLK-PA00/40\nDATA-PA01/41"
				(at 2.54 -13.97 0)
			)
			(text "SPI Flash\nMOSI-PB22/37 \nMISO-PB03/36\nSCK-PB23/38\nCS-PA27/39"
				(at 0 -26.67 0)
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RESET")
				(number "1")
			)
			(pin bidirectional line
				(at 16.51 -52.07 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -29.21 0)
				(length 2.54)
				(name "SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -31.75 0)
				(length 2.54)
				(name "MOSI")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -34.29 0)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin bidirectional line
				(at 16.51 -10.16 180)
				(length 2.54)
				(name "D2")
				(number "14")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "EN")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -44.45 0)
				(length 2.54)
				(name "SWDIO")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -46.99 0)
				(length 2.54)
				(name "SWCLK")
				(number "17")
			)
			(pin bidirectional line
				(at 16.51 -12.7 180)
				(length 2.54)
				(name "D3")
				(number "18")
			)
			(pin bidirectional line
				(at 16.51 -15.24 180)
				(length 2.54)
				(name "D4")
				(number "19")
			)
			(pin power_out line
				(at -17.78 -8.89 0)
				(length 2.54)
				(name "+3V3")
				(number "2")
			)
			(pin bidirectional line
				(at 16.51 -5.08 180)
				(length 2.54)
				(name "D0/RX")
				(number "20")
			)
			(pin bidirectional line
				(at 16.51 -7.62 180)
				(length 2.54)
				(name "D1/TX")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -41.91 0)
				(length 2.54)
				(name "SDA")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -39.37 0)
				(length 2.54)
				(name "SCL")
				(number "23")
			)
			(pin output line
				(at 16.51 -19.05 180)
				(length 2.54)
				(name "D5")
				(number "24")
			)
			(pin bidirectional line
				(at 16.51 -22.86 180)
				(length 2.54)
				(name "D7")
				(number "25")
			)
			(pin bidirectional line
				(at 16.51 -25.4 180)
				(length 2.54)
				(name "D9")
				(number "26")
			)
			(pin bidirectional line
				(at 16.51 -27.94 180)
				(length 2.54)
				(name "D10")
				(number "27")
			)
			(pin bidirectional line
				(at 16.51 -30.48 180)
				(length 2.54)
				(name "D11")
				(number "28")
			)
			(pin bidirectional line
				(at 16.51 -33.02 180)
				(length 2.54)
				(name "D12")
				(number "29")
			)
			(pin input line
				(at -17.78 -21.59 0)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 16.51 -35.56 180)
				(length 2.54)
				(name "D13")
				(number "30")
			)
			(pin power_out line
				(at -17.78 -13.97 0)
				(length 2.54)
				(name "USB")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -52.07 0)
				(length 2.54)
				(name "GND")
				(number "32")
			)
			(pin power_in line
				(at -17.78 -16.51 0)
				(length 2.54)
				(name "VBAT")
				(number "33")
			)
			(pin power_out line
				(at -17.78 -11.43 0)
				(length 2.54)
				(name "VHI")
				(number "4")
			)
			(pin bidirectional line
				(at 16.51 -39.37 180)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin bidirectional line
				(at 16.51 -41.91 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 16.51 -44.45 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 16.51 -46.99 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 16.51 -49.53 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
		)
	)
)